|  |  |
| --- | --- |
|  | **www.QuantumMicrowave.com** |
|  | **P/N: QMC-CRYOTERM-DC40 DC-40 GHz Cryogenic Termination** |
|  | **Features*** Frequency: DC to 40 GHz
* 50 Ohm Load
* Excellent RF Match
* Non-superconducting
* NiCr on Crystalline Quartz
* Silver Epoxy bonded
* Machined OFHC block, gold plated
* 2.92mm male connector
* Stackable mechanical design
* Operates in the mK Temperature Range
 | A picture containing projector  Description automatically generated |
|  |  |  |
|  |

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Specification** | **Notes** |
| Frequency Range | DC to 40 GHz |  |
| Return Loss | 18dB typ. |  |
| Connectors | 2.92mm (m) |  |
| Max Power Handling | 100 mW |  |

**Measured Data, Typical** |
|  |  |

|  |  |
| --- | --- |
|  | **Outline Drawing [inches]** |
|  |  |

**Quantum Microwave Components Phone 857-499-0071, Fax 888-893-7188**