|  |  |  |
| --- | --- | --- |
|  | **www.QuantumMicrowave.com** | |
|  | **P/N: QMC-CRYOTERM-DC40 DC-40 GHz Cryogenic Termination** | |
|  | **Features**   * Frequency: DC to 40 GHz * 50 Ohm Load * Excellent RF Match * Non-superconducting * NiCr on Crystalline Quartz * Silver Epoxy bonded * Machined OFHC block, gold plated * 2.92mm male connector * Stackable mechanical design * Operates in the mK Temperature Range | A picture containing projector  Description automatically generated |
|  |  |  |
|  | |  |  |  | | --- | --- | --- | | **Parameter** | **Specification** | **Notes** | | Frequency Range | DC to 40 GHz |  | | Return Loss | 18dB typ. |  | | Connectors | 2.92mm (m) |  | | Max Power Handling | 100 mW |  |   **Measured Data, Typical** | |
|  |  | |

|  |  |
| --- | --- |
|  | **Outline Drawing [inches]** |
|  |  |

**Quantum Microwave Components Phone 857-499-0071, Fax 888-893-7188**